VITESS Tool Generate Mirror Files

# VITESS Tool Generate Surface Files

This tool generates surface files that are used in the module 'bender'. The following parameters have to be given.

Parameter | Description | Values and range

Number N of channels

The bender can consist of N channels, each of which consists of M wafers.
The wafers of a channel must have the same length, the channels may have different lenghts and a spacing at the exit (see below).
In case of equal lengths and no spacing, there is no difference between L channels a 1 wafer and 1 channel a N wafers.

>= 1

Number M of wafers per channel | Each channel consist of M identical wafers. | >= 1
Thickness of wafer [cm] | Layer thickness of each wafer | > 0
Radius of the bender [cm] | Radius of the middle of the bender. The radius for each wafer is calculated in a way that they all form parts of circles with one common centre. | >= 0 0 = straight
Space between channels at exit [cm] | The channels may be separated by a certain distance at the exit. The distance is supposed to be zero at the entrance and increases linearly over the bender length. | >= 0 0 = no space between channels at exit
File name | Path and name of the file into which the data shall be written. If no path is given, the file will be written to the directory .../Vitess. |

Back to VITESS overview
vitess@helmholtz-berlin.de