description O.K.

Parameter directory is C:/Programme/VITESS_2_5_1/FILES/BEND_DIR
Starting simulation
C:/Programme/VITESS_2_5_1/MODULES/source.exe -S2 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog1 -R60.0 -NSNS -aC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/SnsColdCpld.mod -n1000 -m0.1 -t0 -M5 -T1.2 -d1 -P0 -X0 -Y0 -V1 -D1000 -w2.8 -h5 -k1 -rfermi.out 
| C:/Programme/VITESS_2_5_1/MODULES/bender.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog2 -o3 -h5 -H5 -s0.0001 -l229 -R16400 -iC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr0.dat -mC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr2linear.dat -kC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr1b.dat -IC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr0.dat -MC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr2linear.dat -KC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr1b.dat -uC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/SurfaceT9.dat -g0 -c6 -z1 -w1 -r0.005 -a0 -y1 -p0 -V2 -t0 
| C:/Programme/VITESS_2_5_1/MODULES/monitor1.exe -k5 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog3 -OC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mon_pos_y.dat -n23 -m-0.2875 -M0.2875 -p1 -e0 
| C:/Programme/VITESS_2_5_1/MODULES/monitor1.exe -k3 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog4 -OC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mon_div_y.dat -n40 -m-2 -M2 -p1 -e0 
| C:/Programme/VITESS_2_5_1/MODULES/chopper_fermi.exe -O1 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog5 -X10 -Y0 -V0 -a5 -b4 -c3 -l16 -m0.02 -r8 -n30 -q-55.5 
| C:/Programme/VITESS_2_5_1/MODULES/space.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog6 -d200 
| C:/Programme/VITESS_2_5_1/MODULES/writeout.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog7 -AC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/fermi.out -F1 --Fno_file
simulation (774 fc4 e14 198 ebc fc0 a54 ) (1908 4036 3604 408 3772 4032 2644) is active
....------------------------------


VITESS version 2.5 module Source and Window 1.11

> Simulation of short pulsed spallation source SNS <
pulse frequency              :  60.000 Hz 

coupled moderator
moderator temperature        :  50.000 K
total neutron flux (in 2*pi) : 4.7205e+013 n/(cm²s) 
moderator position           :(  0.000    0.000    0.000) cm 
moderator size (W x H)       :  10.000 cm  x  12.000 cm 
divergence defined by propagation window 
time averaged neutron current: 1.2621e+010 n/s in 0.000014 str
wavelength band used         :   0.100 Ang -   5.000 Ang
time interval used           :   0.000 ms  -   1.200 ms 

window (W x H)               :   2.800 cm  x   5.000 cm 
  in a distance of           :  10.000 m   
  with a declination of      :   0.000°    
polarization                 :   0.000 %  X: 0.000 Y: 0.000 Z: 1.000
trace file used              : fermi.out
Center of beam at window     :(1000.000    0.260    0.238) cm 
Average TOF                  :   5.133 ms 

Gravity is enabled 
Cutoff probability per traj. : 1.000e-006 

number of trajectories started         :        1000
 1 number of trajectories read         :           0
   number of trajectories written      :        1000
(time averaged) neutron count rate     : 9.8739e+009 n/s 
------------------------------


VITESS version 2.5 module Bender 1.6
Inside bender abutment loss is disabled 
The dependance of reflectivity from polarization of neutron is disabled 
The reflected surface is rough 
Minimal weight for tracing neutron   1.000000e-006 
Number of surfaces: 14
entrance: max = 1.400000  min = -1.400000 
exit    : max = 2.000000  min = -2.000000 
BENW= 2.800000  BEXW= 4.000000 
Open visual output device - display+file 
Number of visualised neutrons = 10000 
Magnetic field direction - AXIS OZ 
Inside bender gravity is disabled 
Close graphical window
 2 number of trajectories read         :        1000
   number of trajectories written      :         533
(time averaged) neutron count rate     : 4.0575e+009 n/s 
------------------------------


VITESS version 2.5 module monitor1 1.4
Norm:  1.000000
 3 number of trajectories read         :         533
   number of trajectories written      :         533
(time averaged) neutron count rate     : 4.0575e+009 n/s 
------------------------------


VITESS version 2.5 module monitor1 1.4
Norm:  1.000000
 4 number of trajectories read         :         533
   number of trajectories written      :         533
(time averaged) neutron count rate     : 4.0575e+009 n/s 
------------------------------
 


VITESS version 2.5 module Fermi-Chopper 1.14

Straight Fermi chopper option activated
Channel width: 0.228750 cm
Phase set is -55.500000°.
 
 5 number of trajectories read         :         533
   number of trajectories written      :           4
(time averaged) neutron count rate     : 9.0399e+005 n/s 
------------------------------


VITESS version 2.5 module Space 1.0a
Distance between entrance and exit plane:  200.000  cm 
Center of beam at exit:  ( 200.000,  1.223, -1.334) cm, TOF =   5.8634 ms 
 
 6 number of trajectories read         :           4
   number of trajectories written      :           4
(time averaged) neutron count rate     : 9.0399e+005 n/s 
------------------------------


VITESS version 2.5 module writeout 1.4d
 7 number of trajectories read         :           4
   number of trajectories written      :           4
(time averaged) neutron count rate     : 9.0399e+005 n/s 
------------------------------
Warning: Could not load g2 resource DLL
 Menu and Icon are disabled
simulation finished


