description O.K.

Parameter directory is C:/Programme/VITESS_2_5_1/FILES/BEND_DIR
Starting simulation
C:/Programme/VITESS_2_5_1/MODULES/source.exe -S2 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog1 -R60.0 -NSNS -aC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/SnsColdCpld.mod -n500000 -m0.1 -t0 -M5 -T1.2 -d1 -P0 -X0 -Y0 -V1 -D1000 -w2.8 -h5 -k0 
| C:/Programme/VITESS_2_5_1/MODULES/bender.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog2 -o2 -h5 -H5 -s0.0001 -l17.8 -R927 -iC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr0.dat -mC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr2linear.dat -kC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr1b.dat -IC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr0.dat -MC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr2linear.dat -KC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mirr1b.dat -uC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/SurfaceS1_1.dat -g0 -c6 -z1 -w1 -r0.005 -a0 -y0 -p0 -V2 -t0 
| C:/Programme/VITESS_2_5_1/MODULES/monitor1.exe -k5 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog3 -OC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mon_pos_y.dat -n23 -m-0.2875 -M0.2875 -p1 -e0 
| C:/Programme/VITESS_2_5_1/MODULES/monitor1.exe -k3 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog4 -OC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mon_div_y.dat -n40 -m-2 -M2 -p1 -e0 
| C:/Programme/VITESS_2_5_1/MODULES/chopper_fermi.exe -O1 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog5 -X10 -Y0 -V0 -a5 -b4 -c3 -l16 -m0.02 -r8 -n30 -q-55.5 
| C:/Programme/VITESS_2_5_1/MODULES/monitor1.exe -k1 --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog6 -OC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/mon_lambda2.dat -n50 -m0 -M5 -p1 -e0 -t-1.e10 -T1.e10 
| C:/Programme/VITESS_2_5_1/MODULES/spacewindow.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog7 -l200 -R0 -h-2.5 -H2.5 -w-0.5 -W0.5 -S0 -t0 -c6 
| C:/Programme/VITESS_2_5_1/MODULES/sample_powder.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog8 -D135 -d45 -P180 -p180 -A30 -I0 -SC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/ptest.pow 
| C:/Programme/VITESS_2_5_1/MODULES/detector.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog9 -Gcyl -h200 -w620 -t1 -e0.9 -T180 -P0 -D200 -c310 -r100 -A1 -M0 -g1 
| C:/Programme/VITESS_2_5_1/MODULES/visual.exe --Z1 --G1 --U1.0e-6 --B10000 --PC:/Programme/VITESS_2_5_1/FILES/BEND_DIR --LC:/Programme/VITESS_2_5_1/FILES/BEND_DIR/vpipelog10 -o3 -R2 -m1.95 -M2.0 -h-100 -H100 -w-200 -W200 -k1 --Fno_file
simulation (a58 fd0 e2c eec 254 c28 e24 e3c ba8 904 ) (2648 4048 3628 3820 596 3112 3620 3644 2984 2308) is active
.........................................................------------------------------


VITESS version 2.5 module Source and Window 1.11

> Simulation of short pulsed spallation source SNS <
pulse frequency              :  60.000 Hz 

coupled moderator
moderator temperature        :  50.000 K
total neutron flux (in 2*pi) : 4.7205e+013 n/(cm²s) 
moderator position           :(  0.000    0.000    0.000) cm 
moderator size (W x H)       :  10.000 cm  x  12.000 cm 
divergence defined by propagation window 
time averaged neutron current: 1.2621e+010 n/s in 0.000014 str
wavelength band used         :   0.100 Ang -   5.000 Ang
time interval used           :   0.000 ms  -   1.200 ms 

window (W x H)               :   2.800 cm  x   5.000 cm 
  in a distance of           :  10.000 m   
  with a declination of      :   0.000°    
polarization                 :   0.000 %  X: 0.000 Y: 0.000 Z: 1.000
Center of beam at window     :(1000.000    0.009    0.064) cm 
Average TOF                  :   4.550 ms 

Gravity is enabled 
Cutoff probability per traj. : 1.000e-006 

number of trajectories started         :      500000
 1 number of trajectories read         :           0
   number of trajectories written      :      500000
(time averaged) neutron count rate     : 1.2054e+010 n/s 
------------------------------


VITESS version 2.5 module Bender 1.6
Inside bender abutment loss is disabled 
The dependance of reflectivity from polarization of neutron is disabled 
The reflected surface is rough 
Minimal weight for tracing neutron   1.000000e-006 
Number of surfaces: 71
entrance: max = 1.400000  min = -1.400000 
exit    : max = 1.400000  min = -1.400000 
BENW= 2.800000  BEXW= 2.800000 
Magnetic field direction - AXIS OZ 
Inside bender gravity is disabled 
 2 number of trajectories read         :      500000
   number of trajectories written      :      280629
(time averaged) neutron count rate     : 4.4797e+009 n/s 
------------------------------


VITESS version 2.5 module monitor1 1.4
Norm:  1.000000
 3 number of trajectories read         :      280629
   number of trajectories written      :      280629
(time averaged) neutron count rate     : 4.4797e+009 n/s 
------------------------------


VITESS version 2.5 module monitor1 1.4
Norm:  1.000000
 4 number of trajectories read         :      280629
   number of trajectories written      :      280629
(time averaged) neutron count rate     : 4.4797e+009 n/s 
------------------------------
 


VITESS version 2.5 module Fermi-Chopper 1.14

Straight Fermi chopper option activated
Channel width: 0.228750 cm
Phase set is -55.500000°.
 
 5 number of trajectories read         :      280629
   number of trajectories written      :        4684
(time averaged) neutron count rate     : 8.2160e+007 n/s 
------------------------------


VITESS version 2.5 module monitor1 1.4
Norm:  1.000000
 6 number of trajectories read         :        4684
   number of trajectories written      :        4684
(time averaged) neutron count rate     : 8.2160e+007 n/s 
------------------------------


VITESS version 2.5 module Space and Window 2.21
OUTER MATERIAL OF COLLIMATOR: IDEAL ABSORBER 
Thickness of outer material of collimator 0.000000 cm 
Gravity is enabled 
Distance between plane x=0 and window plane  200.000000 cm 
Center of beam: X = 200.000000 cm Y = 0.070831 cm Z = 0.134932 cm 
 
 7 number of trajectories read         :        4684
   number of trajectories written      :        1351
(time averaged) neutron count rate     : 2.3766e+007 n/s 
------------------------------


VITESS version 2.5 module sample_powder 1.5
Cylindrical sample :    0.50 cm radius  5.00 cm height
  direction        :(   0.000,  0.000,  1.000)   
  position         :(  10.00,   0.00,   0.00 ) cm
macr. cross section:    0.00048,   0.09060,   0.01390  1/cm (incoh, total scat; absorption)
unit cell volume   :   66.380 Ang³
struct. factor file: Al_300.str

 8 number of trajectories read         :        1351
   number of trajectories written      :      153330
(time averaged) neutron count rate     : 5.1541e+005 n/s 
------------------------------


VITESS version 2.5 module detector 1.5
 
 9 number of trajectories read         :      153330
   number of trajectories written      :       66870
(time averaged) neutron count rate     : 1.2203e+005 n/s 
------------------------------


VITESS version 2.5 module visualize 1.02
Open visual output device - display+file 
10 number of trajectories read         :       66870
   number of trajectories written      :       66870
(time averaged) neutron count rate     : 1.2203e+005 n/s 
------------------------------
Warning: Could not load g2 resource DLL
 Menu and Icon are disabled
simulation finished


