# VITESS Tool rvitess

    With this tool you may visualise VITESS output files.
    It reads and displays ASCII output from module writeout, and
    binary output files.

    To read binary files call rvitess on a computer of same convenience as VITESS,
    i.e. the same operating system and hardware architecture.

    This tool assumes you have IDL or PV-Wave software installed
    on your computer.
    If the TOOLS directory is C:/Programs/Vitess/Tools,
    you call it from an idl / pv-wave command window prompt by typing

    cd, 'C:/Programs/Vitess/Tools'
    rvitess

    To call rvitess directly from the VITESS GUI, you have to provide
    a call script in the MODULES directory: rvitess.exe for Windows,
    rvitess_Linux for linux, and so on. The provided rvitess_Linux
    works for the HZB and contains

    #!/bin/sh
    callwave `pwd`/TOOLS rvitess

Back to VITESS overview
vitess@helmholtz-berlin.de