description O.K.

Parameter directory is L:/FILES/ELLI_MIRR_DIR
Starting simulation
D:/Programme/Vitess2-10beta/MODULES/source.exe -S3 --pC:/temp/ics1304695283pgress.txt --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog1 -NESS -L5.0 -R16.667 -p2.0 -aL:/FILES/ELLI_MIRR_DIR/EssLPCold_1x1.mod -n100000 -m4.5 -t0 -y0 -M5.5 -T3 -z0 -d1 -P0 -X0 -Y0 -V1 -D100 -w10 -h10 -i0 -A0 -k0 
| D:/Programme/Vitess2-10beta/MODULES/monitor1.exe -k1 --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog2 -OL:/FILES/ELLI_MIRR_DIR/guide_in.mtl -n100 -C0 -f1 -m0 -M20 -p1 -e0 
| D:/Programme/Vitess2-10beta/MODULES/mon2_pos.exe --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog3 -OL:/FILES/ELLI_MIRR_DIR/source.pos -y80 -z80 -w-4 -W4 -h-4 -H4 -p1 -e0 -F0 -l-1.0 -L21 
| D:/Programme/Vitess2-10beta/MODULES/mirror_elliptical.exe --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog4 -a350 -b7 -c20 -d250 -e0 -k0 -Q0.0 -g0 -A0 -C500 -D-7 -E7 -H-20 -K20 -s500 -t0 -w0 -y1 -Y1 -v0 -l0 -u1 -R0 -iL:/FILES/ELLI_MIRR_DIR/mirr30op10.dat -IL:/FILES/ELLI_MIRR_DIR/mirr30op10.dat -q0 -p0 -V0 -z0 -r55.0 
| D:/Programme/Vitess2-10beta/MODULES/space.exe --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog5 -d100 
| D:/Programme/Vitess2-10beta/MODULES/mon2_pos.exe --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog6 -OL:/FILES/ELLI_MIRR_DIR/dist100.pos -y60 -z100 -w-6 -W6 -h-10 -H10 -p1 -e0 -F0 -l-1.0 -L21 
| D:/Programme/Vitess2-10beta/MODULES/monitor1.exe -k1 --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog7 -OL:/FILES/ELLI_MIRR_DIR/dist100.mtl -n100 -C0 -f1 -m0.2 -M20 -p1 -e1 
| D:/Programme/Vitess2-10beta/MODULES/monitor1.exe -k3 --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog8 -OL:/FILES/ELLI_MIRR_DIR/dist100.mdy -n120 -C0 -f0 -m-3 -M3 -p1 -e1 -l-1.0 -L21 
| D:/Programme/Vitess2-10beta/MODULES/monitor1.exe -k4 --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog9 -OL:/FILES/ELLI_MIRR_DIR/dist100.mdz -n120 -C0 -f0 -m-3 -M3 -p1 -e1 
| D:/Programme/Vitess2-10beta/MODULES/monitor1.exe -k5 --Z1 --U1.0e-25 --G1 --B10000 --PL:/FILES/ELLI_MIRR_DIR --LL:/FILES/ELLI_MIRR_DIR/ics1305105261vpipelog10 -OL:/FILES/ELLI_MIRR_DIR/dist100.mty -n40 -C0 -f0 -m-10 -M10 -p1 -e0 -l-1.0 -L-1.0 --Fno_file
simulation (dd0 18d8 1de4 1268 ec4 10d8 c38 f8 1940 1c14 ) (3536 6360 7652 4712 3780 4312 3128 248 6464 7188) is active
..------------------------------
GSL_RNG_TYPE=ran3
GSL_RNG_SEED=1


VITESS version 2.10  module Source and Window 1.15

> Simulation of long pulse spallation source ESS <
pulse length                 :   2.000 ms 
pulse frequency              :  16.667 Hz 
average power                :   5.000 MW 

Warning: Maximal accelerator current of  60.0 mA exceeds limit of 50.0 mA!
coupled moderator
moderator temperature        :  50.000 K
total neutron flux (in 2*pi) : 1.5342e+014 n/(cm²s) 
moderator position           :(  0.000    0.000    0.000) cm 
moderator size (W x H)       :   1.000 cm  x   1.000 cm 
divergence defined by propagation window 
time averaged neutron current: 2.4376e+011 n/s in 0.009983 str
wavelength band used         :   4.500 Ang -   5.500 Ang
time interval used           :   0.000 ms  -   3.000 ms 

real window    (W x H)       :  10.000 cm  x  10.000 cm
  in a distance of           :   1.000 m
  with a declination of      :   0.000°
polarization                 :   0.000 %  X: 0.000 Y: 0.000 Z: 1.000
Center of beam at window     :(100.000    0.003    0.011) cm 
Average TOF                  :   2.531 ms 

Gravity is enabled 
Cutoff probability per traj. : 1.000e-025 

number of trajectories started         :      100000
 1 number of trajectories read         :           0
   number of trajectories written      :      100000
(time averaged) neutron count rate     : 1.3500e+010 +/- 4.964e+007 n/s 
------------------------------


VITESS version 2.10  module monitor1_wavelength 1.7
Norm     : 0.200000
Binning  : 100 bins from    0.00000 to   20.00000 Ang
File     : L:/FILES/ELLI_MIRR_DIR/guide_in.mtl
total neutron count rate within binning and eval. time: 1.3500e+010 n/s 

 2 number of trajectories read         :      100000
   number of trajectories written      :      100000
(time averaged) neutron count rate     : 1.3500e+010 +/- 4.964e+007 n/s 
------------------------------


VITESS version 2.10  module mon2_pos 1.2b
 3 number of trajectories read         :      100000
   number of trajectories written      :      100000
(time averaged) neutron count rate     : 1.3500e+010 +/- 4.964e+007 n/s 
------------------------------


VITESS version 2.10  module Elliptic Mirror 1.22
Halfaxis of ellipsoid   350.000000   7.000000   20.000000
The reflectivity of the mirror is choosen according refl. files
Only reflected neutrons are going later in the next module
The dependance of reflectivity from polarization of neutron is disabled
The reflected surface is an ideal mirror
Minimal weight for tracing neutron   1.000000e-025
No air attenuation
Magnetic field direction - AXIS OX
Elliptic mirror: Gravity is enabled
 4 number of trajectories read         :      100000
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module Space 1.2
Distance between entrance and exit plane:  100.000  cm 
Center of beam at exit:  ( 100.000,  0.001,  0.066) cm, TOF =  10.1086 ms 
 
 5 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module mon2_pos 1.2b
 6 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module monitor1_wavelength 1.7
Norm     : 0.198000
Binning  : 100 bins from    0.20000 to   20.00000 Ang
File     : L:/FILES/ELLI_MIRR_DIR/dist100.mtl
total neutron count rate within binning and eval. time: 3.8351e+009 n/s 

 7 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module monitor1_horizontal divergence 1.7
Binning  : 120 bins from   -3.00000 to    3.00000 deg
File     : L:/FILES/ELLI_MIRR_DIR/dist100.mdy
total neutron count rate within binning and eval. time: 3.8351e+009 n/s 

 8 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module monitor1_vertical divergence 1.7
Binning  : 120 bins from   -3.00000 to    3.00000 deg
File     : L:/FILES/ELLI_MIRR_DIR/dist100.mdz
total neutron count rate within binning and eval. time: 3.8351e+009 n/s 

 9 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------


VITESS version 2.10  module monitor1_horizontal position 1.7
Binning  : 40 bins from  -10.00000 to   10.00000 cm
File     : L:/FILES/ELLI_MIRR_DIR/dist100.mty
total neutron count rate within binning and eval. time: 3.8351e+009 n/s 

10 number of trajectories read         :       32703
   number of trajectories written      :       32703
(time averaged) neutron count rate     : 3.8351e+009 +/- 2.464e+007 n/s 
------------------------------
simulation finished after 1 s


