This is a description of bugs found in version 2.3.

These bugs have been corrected in the distribution files
if not otherwise stated.


Module Source
-------------
Analytical calculation of the pulse shape from input data 'tau_1' and 'tau_2'
 (pulse shapes calculated from 'tau_1' and 'tau_2' were a factor 1000
 too short due to a missing conversion from ms to s.
 This did not happen, if ESS or SNS were chosen (in any way) to define
 the pulse.)
affected source files: source.c src_modchar.c

Tool DirectView
---------------
Calculation of 'actual curvature' corrected
for case: straight part before bender greater zero
 (The width D of the bender was omitted, i.e.  alpha = L / R_i  was calculated
  instead of  alpha = L /(R_i + D/2)  (L: Length of bender, R_i: inner radius)

  This gave too large values of alpha and therefore too small values for the
  length (of the second straight guide) necessary to prevent direct view.)
affected files: direct_view.c

Tool GenerBatch
---------------
1. BUFLEN increased
    (string was too short for module bender under certain circumstances)
2. subst command improved
    (error occurred if logical drive P: or V: already existed or
         if directory was the root directory (of a drive))
3. MAX_SIM simulations rendered possible
    (number of ll  simulation was limited by MAX_PAR (=15) instead of
    MAX_SIM (=25))
4. deleting tabs in 'GetLine'
    (Apart from comments, line feeds, carriage returns and leading blanks,
     tabs are also removed from the lines read from input files)
5. Improved message at the end of the batch

Additional changes:
1. higher number of possíble files and simulations
    (now 10 files can be copied (instead of 5) and 100 simulations performed
    instead 25)
2. collection of results
    (for files with extension 'col' all data are collected in 'Collect.dat')
affected source files: gener_batch.c gener_batch.html

VITESS GUI
----------
Module rotating_field: You may specify negative values for the
X, Y and Z components of the magnetic field now.
Module mon2_div: angle ranges from -180 to 180 degree are allowed now.
Saving a simulation via Save Instrument / Save As sets the instrument
name - saving to C:\a_something.gui set the name to a_something.
You may change the font used for menubar elements in the GUI now.
affected files:  control.tcl ldstore.tcl menu.tcl tools.tcl vitess.tcl

VITESS documentation
--------------------
Corrected: guide.html
Some files where missing:
ModFlux.gif source1.gif source2.gif LogInterpol.gif
Maxwellian.gif TrajCur.gif gener_batch.html flux_cw.gif
flux_pulse.gif
